**Automatic Engine Termination System**

The Automatic Engine Termination System compares simulation data to actual engine performance. If operation is not in bounds engine terminated.

The metrics compared by the AETS system are pressure and temperature.

Pressure

temperature

time

time

**Process:**

The AETS algorithm compares data at a (timestamp) to equivalent simulation data at its corresponding (timestamp). With an additional grace range (+ 5 / -5). Different data sources are separated into channels where they are independently compared to their associated simulation data. Each channel can contain comparisons with as many as 2 independent data sources.

**Channel 2 – Pressure**

**(2 Comparisons)**

Simulated

Derived

Simulated

Derived

Simulated

Derived

**Channel 1 – Temp**

**(1 Comparison)**

(\*v2 AETS implementing anomaly detection algorithms in analysis)